|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Lanyard Model / Name: | |  | Lot Number: |  | |
| Model / Name: |  | | Date of Manufacturer: | |  |

|  |  |  |  |
| --- | --- | --- | --- |
| Date of Purchase: |  |  |  |

Comments:

|  |
| --- |
|  |
|  |
|  |

|  |  |  |
| --- | --- | --- |
| **General Factors** | **Accepted/Rejected** | **Supportive Details/Comments** |
| 1. **Hardware:** (includes snaphooks, carabiners, adjusters, keepers, thimbles and D-rings) Inspect for damage, distortion, sharp edges, burrs, cracks, corrosion and proper operation. | Accepted  Rejected |  |
| 1. **Webbing:** Inspect for cuts, burns, tears, abrasions, frays, excessive soiling and discoloration. | Accepted  Rejected |  |
| 1. **Stitching:** Inspect for pulled or cut stitches | Accepted  Rejected |  |
| 1. **Synthetic Rope:** Inspect for pulled or cut yarns, burns, abrasions, knots, excessive soiling and discoloration. | Accepted  Rejected |  |
| 1. **Energy Absorbing Component:** Inspect for elongation, tears and excessive soiling. | Accepted  Rejected |  |
| 1. **Labels:** Inspect, making certain all labels are securely held in place and are legible. | Accepted  Rejected |  |
| **Overall Disposition:** | Accepted  Rejected | **Inspected By:**  **Date Inspected:** |

| **Revision / Review History** | | | |
| --- | --- | --- | --- |
| **Revision** | **Date** | **Authorized By** | **Changes** |
| 1 | 9/22/2004 | Safety Director | Annual review |
| 2 | 10/8/2004 | Safety Director | Format Update |
| 2 | 1/3/2006 | Safety Director | Annual review |
| 3 | 6/26/2006 | Safety Director | Minor Update |
| 3 | 10/7/2011 | Safety Director | Annual review |
| 3 | 11/12/2013 | Safety Director | Annual review |
| 3 | 7/18/2016 | Safety Director | Annual review |
| 3 | 6/30/2017 | Safety Director | Annual review |
| 3 | 8/15/2018 | Safety Director | Annual review |
| 3 | 6/10/2019 | Safety Director | Annual review |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |